## horizontal line



Capstone Design Document

Robotic Air Hockey System  
2018.07.09

David Eelman - 6365316  
Stanislav Rashevskyi - 7028178  
Thomas Abdallah - 7141518

Conestoga College

Electronic Systems Engineering  
Capstone Project II - EECE74135

Semester 8, Class of 2018

[horizontal line 0](#_Toc518638416)

[Introduction 2](#_Toc518638417)

[System Description 2](#_Toc518638418)

[Paddle Controller 3](#_Toc518638419)

[Master Controller 5](#_Toc518638420)

[Puck Tracker 5](#_Toc518638421)

[User Interface 5](#_Toc518638422)

[Test Plans 6](#_Toc518638423)

[System Test Plan 6](#_Toc518638424)

[Paddle Controller 6](#_Toc518638425)

[Master Controller 9](#_Toc518638426)

[Puck Tracker 9](#_Toc518638427)

[User Interface 9](#_Toc518638428)

[Risk Analysis 10](#_Toc518638429)

[Appendix 12](#_Toc518638430)

[References 13](#_Toc518638431)

# Introduction

This document will specify the detailed design and test plan of the Robotic Air Hockey System including all subsystems.

# System Description

The Robotic Air Hockey System shall be comprised of two major devices, a robotic system, and the supervisory controller system (Figure 1). The robotic system (referred to as the Paddle Controller) is an embedded system responsible for controlling the movements of the air hockey robot based on commands received over CAN. The supervisory controller system is comprised of three software components, each running as a separate process on a single computer, communicating with each other using inter-process communication.




Figure 1 - System Block Diagram

## Paddle Controller

The Paddle Controller is comprised of three major components, an electro-mechanical system, embedded hardware that interfaces with the electro-mechanical system and the microcontroller, and embedded software running on the microcontroller.

**Electro-Mechanical System**




Figure 2 - Electro-Mechanical System Major Components

The electro-mechanical system (Figure 2) is capable of moving the air hockey paddle in two-axes (Figure 3 - Coordinate System). A single brushed DC motor drives a timing belt to move the air hockey paddle left and right in the X-Axis. Two brushed DC motors driving timing belts are used to move the entire X-Axis assembly forward and backward in the Y-Axis.

A quadrature encoder is mounted to the output shaft of each motor enabling accurate control of speed and position for each motor.

Limit switches are mounted at the end of travel on both ends of each of the three linear rails. If the robot travels outside of the playable area and strikes any limit switch, power to all three motors is shut off to stop the robot from moving any further.

A home position switch (simple micro-switch) is mounted on each of the three linear rails allowing the microcontroller to locate a known “home” position after a reset or during a calibration routine.

Infrared break-beam sensors are installed around the perimeter of the electro-mechanical system to detect intrusions into the robots area of movement. If any of the four break-beam sensors is tripped power to all three motors is shut off to stop the robot from moving any further.

An emergency-stop is installed on the human side of the air hockey table. When pressed, power to all three motors is shut off to stop the robot form moving any further.

**Embedded Hardware**

A custom circuit board serves as the interface between the electro-mechanical system and an off-the-shelf microcontroller (Figure 3).




Figure 3 - Microcontroller Interface Board

The circuit board includes three motor driver circuits allowing each brushed DC motor to be controlled using a single PWM signal from the microcontroller.

Both phases of each of the three quadrature encoders are filtered using a Schmidt trigger. The “A-phase” of each encoder triggers an interrupt on the microcontroller where the “B-phase” of the corresponding encoder is read to determine the direction of rotation for the motor. The “B-phase” of each quadrature encoder is latched on the rising edge of its corresponding “A-Phase” using a D-Flip-Flop to ensure that its value does not change prior to being read during the interrupt-service-routine on the microcontroller.

The infrared (IR) “light screens” (or break-beam sensors) are comprised of an IR LED and an IR sensor that is sensitive to 56 kHz pulses of IR light. The IR LED’s are driven by 555 timers operating in a stable mode outputting a 56 kHz waveform. The IR output of the sensors are filtered using a Schmidt trigger and passed to the microcontroller for processing.

The six limit switch outputs are combined using logical AND-gate, with the output driving the “shutdown” pin on each of the motor driver integrated circuits.

The home switch outputs are filtered using a Schmidt trigger and passed to the microcontroller for processing.

Additional circuitry is included to drive two LED “goal lights” which may be implemented in the future.

**Embedded Software**

An off-the-shelf microcontroller running software written in C is used to interface with the motors and sensors via the embedded hardware. The embedded software communicates with the Master Controller using CAN, transmitting information about the air hockey paddle position, velocity, state, and any error information. The Master Controller sends commands to the embedded software to control the position and velocity of the air hockey paddle, as well as issuing state machine commands (Figure 4).




Figure 4 - Paddle Controller State Machine

## Master Controller

../5_Master_Controller/MC_flowchart.png

Figure 5 - Master Controller Supervisory flowchart

The Master Controller (MC) is responsible for game strategy control, trajectory predictions, data logging and supervisory control. MC process is written in Python 2.7 and ran on off-the-shelf Linux Computer (i7, 16Gb RAM, Ubuntu 14.04).

Figure 5 demonstrates the constant MC program flow:

**Rx IPC and Tx IPC data**

MC establishes inter-process communication with the Puck Tracker (PT) and the User Interface (UI) processes through Python process-based “threading” interface called *multiprocessing*.

Using multiprocessing MC creates two arrays (multiprocessing.Array together with enumerations specified in a JSON file) and a queue (multiprocessing.Queue) for communication with the PT.

PT transmit array is mainly used to identify the velocity and position of the puck on the playing surface, as well as to show current states and errors of the process. Receive array is used to configure the web-camera and change PC states. Visualization receive queue is used to pass camera video stream to the MC.

Using multiprocessing MC creates two arrays (multiprocessing.Array together with enumerations specified in a JSON file) ) and a queue (multiprocessing.Queue) for communication with the UI. UI transmit array is mainly used to identify current menu page, and send data relevant to that page (e.g. diagnostics interface, manual game paddle positions, settings values, etc), as well as to show current states and errors of the process. Receive array is used to change UI states, list current states and errors of other modules, send scored goals, etc. Visualization transmit queue is used to pass camera video stream with drawn game strategy decisions (puck trajectory predictions, paddle movement, etc.) to the UI.

**Rx CAN and Tx CAN data**

Master Controller communicates with the Paddle Controller board using CAN bus, receiving information about the air hockey paddle position, velocity, goals, state, and any error information. The Master Controller transmits commands to the embedded software to control the position and velocity of the air hockey paddle, as well as issuing state machine commands (Figure 4).

**Log Data**

All received and transmitted messages are stored in HDF5 file and analyzed in Matlab. Debug information is stored in a text file using Python *logging* module.

**Analyze Rx data and Make decision**

In data analysis, MC tracks states, errors, quit requests, game modes, and settings. Then MC makes decisions: calculates paddle position for the automated game; handles manual game (paddle position is filtered and sent from the UI touch display); updates settings; calibrates camera; resolves errors and quit requests, etc.




Figure 6 - Complex Defense Algorithm for Automated game

Complex Defense Algorithm for Automated game is shown in Figure 6. Its main purpose is to make sure that paddle defends the goal boundaries at all cost, it has no offensive strategy. An equation of a line (y = mx + b) is a fundamental math concept that lies underneath Calculate Predicted Paddle Position step of the Defense Algorithm. PT from two consecutive camera frames determines two puck position values on the playing surface, this gives us X and Y vectors. Afterward using y = mx + b algorithm predicts the trajectory and final position of the moving puck (e.g. when y = 0). Next, each camera frame allows us to average out trajectory and position calculations to improve accuracy.

Offense Algorithm for Automated game is still under development and will depend on the speed, precision, reaction time of the high-speed Paddle Controller system. This algorithm remains the primary risk for the Master Controller, due to the inexperience with advanced control algorithms and dependency on the Paddle Controller electro-mechanical design.

## Puck Tracker

## User Interface

# Test Plans

## System Test Plan

|  |  |  |
| --- | --- | --- |
| **Test** | **Purpose** | **Expected Result** |
| Defense Test   1. Power on system. 2. Select “defense” from game mode settings in UI. 3. Start game from UI. | Verify operation of defense operating mode. | Air hockey paddle moves in X-Axis only to stop human from scoring goals. |
| Offense Test   1. Power on system. 2. Select “offense” from game mode settings in UI. 3. Start game from UI. | Verify operation of offense operating mode. | Air hockey paddle moves in X and Y-Axis to stop human from scoring goals and to attempt to score goals on the human. |
| Manual Control Test   1. Power on system. 2. Select “manual control” from game mode settings in UI. 3. Start game from UI. | Verify operation of manual control mode. | Air hockey paddle moves in X and Y-Axis following manual control movement on touch-screen. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Paddle Controller

**Electro-Mechanical System Test Plan**

|  |  |  |
| --- | --- | --- |
| **Test** | **Purpose** | **Expected Result** |
| X-Axis motor test   1. Apply 24V to positive motor terminal, GND to negative motor terminal 2. Apply GND to positive motor terminal, 24V to positive motor terminal. | Verify operation of the X-Axis motor. | 1. Paddle moves to the right. 2. Paddle moves to the left. |
| Y-Axis motor test   1. Apply 24V to positive motor terminals, GND to negative motor terminals 2. Apply GND to positive motor terminals, 24V to positive motor terminals. | Verify operation of the Y-Axis motors. | 1. Paddle moves forward. 2. Paddle moves backwards. |
| Quadrature encoder test (x3)   1. Rotate motor clockwise 2. Rotate motor counter-clockwise   Repeat for each of the three quadrature encoders. | Verify operation of the quadrature encoders. | 1. “B-phase” output is low (0V) on each “A-phase” output rising edge (0-5V transition). 2. “B-phase” output is high (5V) on each “A-phase” output rising edge (0-5V transition). |
| Limit switch test (x6)   1. Press the limit switch 2. Release the limit switch   Repeat for each of the six limit switches. | Verify operation of the limit switches. | 1. Limit switch terminals short-circuited. 2. Limit switch terminals open-circuited. |
| Home switch test (x3)   1. Press the home switch 2. Release the home switch   Repeat for each of the three home position switch. | Verify operation of the home position switches. | 1. Home switch terminals short-circuited. 2. Home switch terminals open-circuited. |
| Infrared break-beam sensor test (x4)   1. Obstruct path of break beam sensor with solid object 2. Do not obstruct path of break beam sensor   Repeat for each of the four break-beam sensors. | Verify operation of the break-beam sensors. | 1. IR sensor output is low (0V). 2. IR sensor output is high (5V). |
| Emergency stop test   1. Press the emergency stop 2. Release the emergency stop | Verify the operation of the emergency stop. | 1. 0V applied to both terminals of all three motors. 2. 0-24V applied to both terminals of all three motors. |

**Embedded Hardare Test Plan**

|  |  |  |
| --- | --- | --- |
| **Test** | **Purpose** | **Expected Result** |
| Power supply test   1. Apply 24V and Ground to power input connector. | Verify operation of the 15V and 5V regulators. | V24V power rail measures 24VDC +/- 0.25VDC.  V15V power rail measures 15VDC +/- 0.1VDC.  V5V power rail measures 5VDC +/- 0.1VDC. |
| Motor test (x3)   1. Apply 50% duty cycle PWM waveform to input of motor driver circuit. 2. Apply 95% duty cycle PWM waveform to input of motor driver circuit. 3. Apply 5% duty cycle PWM waveform to input of motor driver circuit.   Repeat of each of the three motor driver circuits. | Verify operation of the motor driver circuits. | 1. Average DC voltage measured between motor driver positive and negative outputs = 0VDC +/- 0.25VDC. 2. Average DC voltage measured between motor driver positive and negative outputs = 21.6VDC +/- 0.25VDC. 3. Average DC voltage measured between motor driver positive and negative outputs = -21.6VDC +/- 0.25VDC. |
| Quadrature encoder test (x6)   1. Apply 0-5VDC square wave to A-phase and B-phase inputs.   Repeat for each of the three quadrature encoder interface circuits. | Verify operation of the quadrature encoder interface circuits. | A-phase output is inverted copy of A-phase input. B-phase output is “latched” value of B-phase input for each A-phase rising edge. |
| Limit switch test (x6)   1. Short-circuit the limit switch output pins. 2. Open-circuit the limit switch output pins.   Repeat for each of the six limit switch interface circuits. | Verify operation of the limit switch interface circuits. | 1. Motor driver “shutdown” pin measures 0VDC. 2. Motor driver “shutdown” pin measures 5VDC. |
| Home switch test (x3)   1. Short-circuit the home switch output pins. 2. Open-circuit the home switch output pins.   Repeat for each of the three home switch interface circuits. | Verify operation of the home switch interface circuits. | 1. Home output pin measures 5VDC. 2. Home output pin measures 0VDC. |
| IR LED driver test (x6)   1. Measure output to IR LED.   Repeat for each of the six IR LED driver circuits. | Verify operation of the IR LED driver circuits. | 1. IR LED positive output is 56 kHz +/- 2 kHz square wave at 0-5VDC. IR LED negative output is grounded. |
| IR sensor test (x6)   1. Apply 5V to IR sensor input pin. 2. Apply 0V to IR sensor input pin.   Repeat for each of the six IR sensor interface circuits. | Verify operation of the IR sensor interface circuits. | 1. IR sensor output pin measures 0VDC. 2. IR sensor output pin measures 5VDC. |

**Embedded Software Test Plan**

|  |  |  |
| --- | --- | --- |
| **Test** | **Purpose** | **Expected Result** |
| Motor test (x3)   1. Command positive X-Axis movement. 2. Command negative X-Axis movement. 3. Command positive Y-Axis movement. 4. Command negative Y-Axis movement. | Verify operation of the motor control software. | 1. X-Axis motor PWM output is >50% duty cycle. 2. X-Axis motor PWM output is <50% duty cycle. 3. Y-Axis motor PWM outputs are >50% duty cycle. 4. Y-Axis motor PWM outputs are <50% duty cycle. |
| Quadrature Encoder test (x3)   1. Rotate motor clockwise. 2. Rotate motor counter-clockwise.   Repeat for each of the three motors. | Verify operation of the quadrature encoder software. | 1. Motor position variable increases. 2. Motor position variable decreases. |
| Home switch test (x3)   1. Press home position switch   Repeat for each of the three home position switches. | Verify operation of the home position switch software. | 1. Motor position variable is reset to its default value (varies depending on motor). |
| Infrared break-beam sensor test (x4)   1. Obstruct path of break-beam sensor with solid object   Repeat for each of the four break-beam sensors. | Verify operation of the break-beam sensor software. | 1. PWM output to all three motors are 50% duty cycle (i.e. off). |
| State machine test   1. Reset microcontroller 2. Obstruct path of any break-beam sensor with a solid object. 3. Stop obstructing all break-beam sensors. Send state command “CLEAR\_ERROR” over CAN. 4. Send state command “ON” over CAN. 5. Send state command “CALIBRATION” over CAN. 6. Send state command “OFF” over CAN. | Verify operation of the Paddle Controller state machine software. | 1. State = “OFF” 2. State = “ERROR” 3. State = “OFF” 4. State = “CALIBRATION”, homing routine begins. State = “ON” after homing routine is complete. 5. State = “CALIBRATION”, homing routine begins. State = “ON” after homing routine is complete. 6. State = “OFF” |

## Master Controller

|  |  |  |
| --- | --- | --- |
| CAN bus test   1. Transmit MC\_Cmd\_PC (value 0x04030201) message over CAN bus 2. Receive PC\_Status (value 0x01020304) message over CAN bus | Verify communication protocol with Paddle Controller over CAN bus | MC receives PC\_Status = “0x01020304”  PC receives MC\_Cmd\_PC = “0x04030201” |
| IPC with PT test   1. Change each value in pt\_tx array 2. Change each value in pt\_rx array 3. Move web-camera | Verify communication protocol with Puck Tracker using Python multiprocessing array and queue and logging | 1. See changes in pt\_tx signals under HDF5 file 2. See changes in pt\_rx signals under HDF5 file 3. Video stream on UI display has changed within 0.3 s |
| IPC with UI test   1. Change each value in ui\_tx array 2. Change each value in ui\_rx array 3. Move web-camera | Verify communication protocol with User Interface using Python multiprocessing array and queue and logging | 1. See changes in ui\_tx signals under HDF5 file 2. See changes in ui\_tx signals under HDF5 file 3. Video stream on UI display has changed within 0.3 s |
| Defense Algorithm test   1. Hit puck to move to the left of goal area 2. Hit puck to move to the right of goal post 3. Hit puck to move into the goal boundaries 4. Repeat above steps with multiple bounces | Verify defense algorithm | 1. Paddle travels to the left goal post 2. Paddle travels to the right goal post 3. Paddle blocks the oncoming puck within the goal boundaries 4. Paddle should react the same as above |
| Offense Algorithm test   1. Place puck on the robot half of the table 2. Hit puck towards to robot 3. Hit puck towards to robot with multiple bounces | Verify offense algorithm | * 1. Paddle hits the puck to go within the opponent’s goal boundaries |
| Error and quit handling test   1. Disconnect Webcam 2. Turn off Paddle Controller 3. Reconnect Webcam 4. Turn on Paddle Controller 5. Press quit under UI 6. Start the MC | Verify error and quit handling | 1. UI diagnostics shows error under PT state 2. UI diagnostics shows that PC is off 3. UI diagnostics shows that PT is active 4. UI diagnostics shows that PC is ON 5. All processes terminated 6. UI diagnostics shows that PT, PT, MC are active |

## Puck Tracker

## User Interface

# Risk Analysis

Addresses safety, societal and environmental issues more or less adequately

States the remaining significant risks and provides a risk management plan somewhat clearly

MC risks are also touched under System description.

Based on the risks we have evaluated in the table below, we have determined that the overall risk for this project is low.

|  |  |  |  |
| --- | --- | --- | --- |
| Risk (Priority Highest to Lowest) | Category | Impact on Project Objectives | Potential Risk Reduction |
| 1. Mechanical design/integration problems | Technical | Unable to control robot motion | -Start mechanical prototyping early  -Leverage group members Mechanical Engineering experience |
| 2. Real-time object tracking problems | Technical | Unable to automate robot motion | -Start object tracking prototyping early  -Leverage proven open-source object tracking solutions |
| 3. Security of project in shared classroom | External | Lack of lab workspace availability.  Potential damage to project hardware. | -Utilize dedicated ESE lab space  -Advocate for continued support of ESE dedicated lab space |
| 4. Catastrophic loss of data | Organizational, external, technical | Schedule delays. | -Utilize source control for all project materials  -Manually back up all data once per week |
| 5. Managing scope creep | Organizational, project management | Schedule delays.  Lack of focus on core features. | -Strictly define scope of project during planning phase  -Additional features shall only be implemented after 100% completion of core project features |
| 6. System sizing incorrect | Technical, performance | Lower than desired system performance. | -Use system level performance requirements to drive component design  -Define system level performance requirements based on real-world data |
| 7. Inexperience with HMI design & implementation | Technical | Less relatable demonstration.  Worse user experience.  Difficult to debug. | -Define user interface features early (see: Managing scope creep)  -Start HMI prototyping early  -Utilize popular GUI implementation solutions |

# Appendix




Figure 7 - Coordinate System

# References

[1] "Air Hockey Robot (a 3D printer hack)", *jjrobots*, 2018. [Online]. Available: https://www.jjrobots.com/air-hockey-robot-a-3d-printer-hack/. [Accessed: 08- Feb- 2018].

[2] "AIR HOCKEY ROBOT EVO - jjrobots", *jjrobots*, 2018. [Online]. Available: https://www.jjrobots.com/the-open-source-air-hockey-robot/. [Accessed: 08- Feb- 2018].

[3] "Multiple Objects Positioning and Identification Method Based on Magnetic Localization System - IEEE Journals & Magazine", *Ieeexplore.ieee.org*, 2018. [Online]. Available: http://ieeexplore.ieee.org/document/7496898/. [Accessed: 08- Feb- 2018].

[4] H. Parekh, D. Thakore and U. Jaliya, "A Survey on Object Detection and Tracking Methods", *International Journal of Innovative Research in Computer and Communication Engineering*, vol. 2, no. 2, 2018.

[5] S. A ̊gren, *Object tracking methods and their areas of application: A meta-analysis*. 2018.

[6] "Create an Object Tracking System: Integrating Servo Control with Object Detect", *Allaboutcircuits.com*, 2018. [Online]. Available: https://www.allaboutcircuits.com/projects/create-an-object-tracking-system-integrating-servo-control-with-object-dete/. [Accessed: 08- Feb- 2018].

[7] W. Hamlet and W. Kusewich, "Using The Ultrasonic Sensor to Determine Location", *Engineering.nyu.edu*, 2018. [Online]. Available: http://engineering.nyu.edu/mechatronics/summit/SUMMIT2007/group6-Will\_Bill/Summit2007Project.pdf. [Accessed: 08- Feb- 2018].

[8] "Motors and Selecting the Right One", *Learn.sparkfun.com*, 2018. [Online]. Available: https://learn.sparkfun.com/tutorials/motors-and-selecting-the-right-one. [Accessed: 08- Feb- 2018].

[9] "Linear Positioning - Motion Control Application", *Oriental Motor U.S.A. Corp.*, 2018. [Online]. Available: http://www.orientalmotor.com/applications/linear-positioning.html. [Accessed: 08- Feb- 2018].

[10] "Know Your Pneumatics: Linear Actuators", *Blog.parker.com*, 2018. [Online]. Available:   
 http://blog.parker.com/know-your-pneumatics-hints-tips-for-specifying-linear-actuators.   
 [Accessed: 08- Feb- 2018].